**Sturdy and Strong**

TAU XTRACTORTM: The ground-breaking discharging solution for lubricants in the mining and steel industries is here

JAKOBSTAD, Finland, March 28, 2019 – Fluid-Bag has been producing innovative bulk packaging and discharge equipment for the global lubricants industry since 1984. Whether it’s an IBC made out of soft plastic never seen on the market before, or the reinvention of a new method of discharging grease, Fluid-Bag is always cutting-edge.

Designing custom-made solutions is the company’s DNA, so the requests from clients for a sturdy discharge device with optimized features for the lubricant and mining industry was a challenge Fluid-Bag accepted. Behind the TAU XTRACTOR lies a two-year innovation process that exceptionally meets the clients’ requirements.

The TAU XTRACTOR uses a completely new method for discharging grease from Fluid-Bag’s flexible containers with benefits optimized for demanding heavy-duty work environments. Exceptionally strong and sturdy, it can withstand harsh treatment in the maintenance area of a mine or a steel plant. The device grips the inner container of the Fluid-Bag, twists it with great strength and forces out the grease, leaving down to 1 % residue in the bag.

Fluid-Bag has always focused on safety and lubricant cleanliness. The TAU XTRACTOR discharge mechanism is fully enclosed behind metal safety doors to protect the container inside. Due to the sealed Fluid-Bag, grease is kept clean from dust, particles and moisture.

“We have taken focusing on safety to another level with this product, since we know how crucial a safe work environment is to all our customers. Since the discharge procedure occurs behind closed safety doors, there is no risk of injury for the user, and the working area is kept clean,” CEO Jan Backman explains.

This method boasts up to 5 times more efficient handling than using traditional drums and

grease pumps. One Fluid-Bag holds 1000 liters of grease, instead of 5 drums of 200 liters each. The TAU XTRACTOR will independently discharge all the grease from the Fluid-Bag at the rate you require, eliminating the need to switch containers every 200 liters.

“We are very proud of the patent pending TAU XTRACTOR, since we know that this reinvention of ours will give our customers an easy and reliable discharge method, a safer product with zero contamination and more cost-effective results,” says Sales Manager Henrik Kass.

**THE STORY BEHIND THE NAME:**

The name and logo TAU XTRACTOR were inspired by the Greek letter Tau (Ꚍ). The symbol Ꚍ is used to represent torque, the force that twists and squeezes the bag.

**About Fluid-Bag**

Fluid-Bag is an innovative player in the heavy-duty industry, manufacturing flexible bulk packaging solutions for liquids and semi-solids. The company’s 72 employees are mainly located in the headquarters in Jakobstad, Finland, with subsidiaries in the USA and Thailand. Fluid-Bag also has a vast network of representatives in Australia, Brazil, China, France, India, Italy, Israel, Netherlands, Norway, Poland, Philippines, South Korea, Spain, Switzerland, and Turkey.

**Henrik Kass**

**Sales Manager, Lubricants**

+358 20 779 0449

[henrik.kass@fluid-bag.com](mailto:henrik.kass@fluid-bag.com)

**Charlotte Sandström**

**Marketing Manager**

+358 20 779 0452

[charlotte.sandstrom@fluid-bag.com](mailto:charlotte.sandstrom@fluid-bag.com)

**Read more:**

* Fluid-Bag containers for lubricants: <https://www.fluid-bag.com/lubes>
* Tau Xtractor: [www.fluid-bag.com/tau-xtractor](http://www.fluid-bag.com/tau-xtractor)
* Download Tau Xtractor product sheet: <https://www.fluid-bag.com/assets/Uploads/Product-Sheet-Tau-Xtractor-ID-37211.pdf>

Images available for download: <https://adobe.ly/2BXEo1a>